1. Section 102600   
   Wall and Door Protection
   1. PART 1  GENERAL
      1. SUBMITTALS
         1. See Section 013000 - Administrative Requirements for submittal procedures.
         2. Product Data:  Indicate physical dimensions, features, wall mounting brackets with mounted measurements, anchorage details, and rough-in measurements.
   2. PART 2  PRODUCTS
      1. PRODUCT TYPES
         1. Corner Guards - Surface Mounted:
            1. Material:  High impact vinyl with full height extruded aluminum retainer.
            2. Material:  Polyethylene terephthalate (PET or PETG); PVC-free with full height extruded aluminum retainer.
            3. Width of Wings:  2 inches.
            4. Corner:  Square.
            5. Color:  As selected from manufacturer's standard colors.
            6. Length:  One piece.
      2. FABRICATION
         1. Fabricate components with tight joints, corners and seams.
   3. PART 3  EXECUTION
      1. INSTALLATION
         1. Install components in accordance with manufacturer's instructions, level and plumb, secured rigidly in position to supporting construction.
         2. Position corner guard ​4 inches​ above finished floor to ​48 inches high​.
2. END OF SECTION

This page intentionally left blank